Fire Pump Operation
These are the basics for setting up, starting and running the fire pump
SETUP
1. Place the pump on a solid surface, close enough for the SUCTION HOSE to reach the water.
2. Check there is gas in the tank.
3. Prime pump - add water into prime port until it exits inlet port (use jug or boat bailer)
4. Attach the SUCTION HOSE to the pump INLET and lock in place. 
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5. Completely submerge the STRAINER in the water – may need weighing down.
6. Unroll the DISCHARGE HOSES, make sure there are no twists or kinks.
7. Attach the female hose end to the pump OUTLET, lock in place.
a. Multiple discharge hoses can be coupled together.
8. Attach the NOZZLE to the end of the discharge hose(s) and lock in place.
9. Prime pump via prime port – use lake water/boat bailer/cup etc – replace prime cap
PRIME PORT
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You are ready to start the engine! Have someone holding the nozzle!

STARTING THE PUMP (TGIC)
Note: pumps in tubular metal cages do NOT have a gas on/off or an ignition switch
Throttle    /    Gas    /    Ignition    /    Choke
Throttle to the left
Gas to the right
Ignition to the “ON” position
Choke to the leftTHROTTLE
CHOKE
IGNITION
GAS
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· Pull the starter cord until pump starts.
· Move the choke to the right. 
· The pump will self-prime up the suction hose if you added water to the pump via priming port, it takes a minute!
· Have someone hold the nozzle, it’s powerful once the water flows!
· Aim water at the base of the fire, adjust nozzle spray pattern as needed
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Moon American, Fire Hose Fog Nozzle, 517-071, 3/4” NPSH, Lexan
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